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	SciAps & detectORE™
	

	
	The Future of In-field Gold Analysis
	

	
	The detectORE App provides highly optimized calibrations for low-level gold analysis anywhere, and it's now available with the best handheld
analyzer ever made, the SciAps X-505.
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	SciAps X-505 handheld XRF with
	

	
	detectORE™ App
	

	
	Data from samples representing a wide variety of gold deposits show an impressive correlation between the detectORE method run on the X-505 and fire assay, from 8.6ppm all the way down to 44ppb. Historically, pXRF has achieved a best-case limit of detection for Au around 1-2ppm but struggled with spectral interferences from elements like Zn, As, W which could decrease accuracy and cause false detections. The detectORE method
lowers the detection limit to 20ppb while virtually eliminating the spectral interferences.
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	SciAps XRF pairs with
	

	
	Portable PPB
	

	
	After several years of working with Portable PPB, SciAps, Inc. is now pleased to offer a fully integrated solution for our clients. SciAps X-505 has been optimized to meet Portable PPB's
stringent requirements, and now has their endorsement to use their unique detectORE™ technique. SciAps is committed to continuing development to further enhance the pXRF capabilities related to this powerful new approach to low-level gold analysis.
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	detectORE App now available on
	

	
	SciAps pXRF
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	detectORE™ is a World First technique exclusive to Portable PPB Pty Ltd for enabling low-level gold analysis from anywhere using the patented detectORE™ Widget, proprietary software and fully optimized portable XRF linked to their pLIMS™ software with full QAQC and tracking. It is a system and a process. The system involves the sample preparation, sample processing and use of a pXRF to obtain low-level gold results in the field. It is a process, that enables rapid progress through “reactive sampling” whereby the explorer can change the sample spacing as results come to hand on a
daily basis. This helps to quickly define and delineate gold anomalies across a range of sample media, which enables explorers to Explore Smarter and Discover Faster™.
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	The detectORE™ process
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	Complete anywhere!
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	Low-level gold by using the SciAps X-505 pXRF is now fully optimized to the patented detectORE™. This provides geologists the ability to detect gold in samples, anywhere, down to low ppb concentrations, whilst not affecting the ability to also collect conventional multi-element results via conventional pXRF processes. Together, transforming the way you explore, define and mine gold.
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	The SciAps X-505 pXRF offers the only way to find economically viable gold concentrations in the field.
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SciAps X-505 handheld XRF with
detectORE™ App

Data from samples representing a wide variety
of gold deposits show an impressive
correlation between the detectORE method
run on the X-505 and fire assay, from 8.6ppm
all the way down to 44ppb. Historically, pXRF
has achieved a best-case limit of detection for
Au around 1-2ppm but struggled with spectral
interferences from elements like Zn, As, W
which could decrease accuracy and cause
false detections. The detectORE method
lowers the detection limit to 20ppb while
virtually eliminating the spectral interferences.
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SciAps XRF pairs with
Portable PPB

After several years of working with Portable PPB, SciAps, Inc. is
now pleased to offer a fully integrated solution for our clients.
SciAps X-505 has been optimized to meet Portable PPB's
stringent requirements, and now has their endorsement to use
their unique detectORE™ technique. SciAps is committed to
continuing development to further enhance the pXRF
capabilities related to this powerful new approach to low-level
gold analysis.
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detectORE App now available on
SciAps pXRF
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detectORE™ is a World First technique exclusive to Portable  .i.ci0mr App now available on
PPB Pty Ltd for enabling low-level gold analysis from anywhere SciAps pXRE

using the patented detectORE™ Widget, proprietary software and fully optimized portable XRF
linked to their pLIMS™ software with full QAQC and tracking. It is a system and a process. The
system involves the sample preparation, sample processing and use of a pXRF to obtain low-
level gold results in the field. It is a process, that enables rapid progress through “reactive
sampling” whereby the explorer can change the sample spacing as results come to hand on a
daily basis. This helps to quickly define and delineate gold anomalies across a range of sample
media, which enables explorers to Explore Smarter and Discover Faster™.
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Low-level gold by using the SciAps X-505 pXRF is now fully optimized to
the patented detectORE™. This provides geologists the ability to detect
gold in samples, anywhere, down to low ppb concentrations, whilst not
affecting the ability to also collect conventional multi-element results
via conventional pXRF processes. Together, transforming the way you
explore, define and mine gold.
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The SciAps X-505 pXRF offers the only way to find economically viable
gold concentrations in the field.
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SciAps & detectORE™ -
The Future of In-field Gold Analysis

The detectORE App provides highly
optimized calibrations for low-level
gold analysis anywhere, and it's now
available with the best handheld
analyzer ever made, the SciAps X-505.
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