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	RoHS
	

	
	Halogen-Free and Restricted Substances App
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	World’s lightest, fastest analyzer for RoHS application
	

	
	The ONLY HH XRF for RoHS, CPSIA, CA Prop 65, Halogen-Free, Environmental Soil (all RCRAs and EPA Priority Pollutant Metals except Be) and HUD/EPA accepted lead based paints (X-550 Pb only).
	

	
	Next-generation connectivity, test data management, barcode reading capabilities, and reporting for the full range of compliance testing applications, including RoHS, Halogen Free, CPSIA, and lead paint in children’s playgrounds.
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	X-505
	

	
	Ultimate X-ray Analysis
	

	
	At 2.75 lbs., it’s the lightest weight analyzer ever created, in a mostly metal frame for ultimate durability and duty cycle. Perfectly balanced and fast– you can test material all day long without fatigue. The narrow, slender form factor accesses the toughest test locations, with the latest 2.7″ (68.6mm) display for rear viewing of chemistry.
	

	[image: ]
	X-200
	

	
	Performance and Value
	

	
	Competitively priced for every performance requirement, this platform weighs about 3.4 lbs., making it about 0.5 lbs. heavier than the X-550 platform, but still with industry leading speed and precision. Updated for improved heat dissipation, reduced weight, new user-interface. All internal electronics now use less power and operate at higher temperatures — no drift or shutdown.
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	X-50
	

	
	Great Basic Analysis
	

	
	A cost effective SDD detector processes about 10x lower X-ray count rates than SDD, resulting in a 3x reduction of precision. However, for many RoHS/WEEE applications, the performance is satisfactory, and the X-50 is available at a lower price point. Includes the same advanced X-ray tube (operating at 50 kV max.), integrated camera, video, and Android platform.
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	Quick, Easy Compliance
	

	
	XRF is an approved analytical technique for screening various products for compliance testing, It’s the quickest and easiest way to pass/fail your products.
	

	
	For RoHS, SciAps instruments comply with IEC 62321-3-1 and ASTM F2617-15, the official methods that describe procedures for the analysis of lead, cadmium, chromium, mercury, and total bromine by XRF. There are additional classifications, like Green for RoHS, which means complying with RoHS as well as restricting flame retardants containing Cl, Br and Sb. SciAps software allows for the ability to add elements like Sb and adjust pass/fail levels to what the customer requires. SciAps instruments can also be used in screening for ASTM F963 compliance, an important standard for toy safety.
	

	
	SciAps engineers have been solving for RoHS from the beginning, through their roles at various companies. We have decades of experience designing the next generation of instruments to meet the growing needs of this market. We bring the best possible screening program to our customers based on accuracy, efficiency, and value for the customer.
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	Future-Proof Your Instrument
	

	
	SciAps RoHS app allows for the greatest customization in the industry. Take back control of your instrument. As regulations increase, you can add elements like Ni, Sb, Ba, and others. Want tighter Pass/Fail requirements? Decrease levels to meet your own more stringent guidelines. No need to buy additional software or a new instrument. Just change settings and you’re ready for any new regulation.
	

	
	Ease of Use — the RoHS App
	

	
	With years of experience in the RoHS market, SciAps designs software with the user in mind. Our automatic identification of material assures that no matter what sample is placed in front of the window, the results will be right. No need for changing back and forth between different modes, calibrations, or applications. The simple-to-use RoHS app does it all.
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	The Best Value for Your Money
	

	
	Testing 4 ppm Cd with a Si Pin was unheard of a decade ago. Advancements in digital pulse processing and the extensive XRF experience at SciAps have produced the best value for money in the industry. While most instruments in the market have changed very little since RoHS or CPSIA was first introduced, SciAps newly software takes modern manufacturing into account.
	

	
	State-of-the-art data management incorporated into a flexible Android system allows for the greatest customization and data management capabilities
	

	
	Redesigned housing with improved heat dissipation allows for high throughput testing that our compliance customers demand.
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	2010 SDD
	

	
	2010 Si PiN
	

	
	SciAps X-50 PiN
	

	
	Tube Power
	

	
	4 W
	

	
	4 W
	

	
	5 W
	

	
	keV
	

	
	40 keV
	

	
	40 keV
	

	
	50 keV
	

	
	Max uA
	

	
	100 uA
	

	
	100 uA
	

	
	200 uA
	

	
	Detector
	

	
	SDD
	

	
	Si Pin
	

	
	Si Pin
	

	
	Processing Speed
	

	
	300-500 MHz CPU,128-500 MB RAM
	

	
	300-550 MHz CPU,128-500 MB RAM
	

	
	1.2 GHz CPU,1 GB RAM
	

	
	Compliance Testing
	

	
	Testing Time
	

	
	120 sec
	

	
	120 sec
	

	
	60 sec
	

	
	Typical Alloy Test
	

	
	120 sec
	

	
	300 sec
	

	
	60 sec
	

	
	LOD: Polymer Pb
	

	
	2-5 ppm
	

	
	3-10 ppm
	

	
	2 ppm
	

	
	LOD: Polymer Cd
	

	
	30-50 ppm
	

	
	30-50 ppm
	

	
	4 ppm
	

	
	LOD: Polymer Cr
	

	
	40-60 ppm
	

	
	30-60 ppm
	

	
	2 ppm
	

	
	LOD: Polymer Cl
	

	
	0.1-0.3%
	

	
	0.5-1%
	

	
	60 ppm
	

	
	LOD: Cu Alloy Cd
	

	
	60-90 ppm
	

	
	60-80 ppm
	

	
	8 ppm
	

	
	LOD: Sn Alloy Pb
	

	
	60-90 ppm
	

	
	120-150 ppm
	

	
	80 ppm
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	Full-Beam Collimation
	

	
	Why spend more for collimation just to receive 1/8th the power? SciAps XRF tight geometry and advanced design allows for a 4 mm beam spot without the need for a collimator. Collimators block X-rays to get the small beam size. This reduces the number of X-rays going into the samples and thus increases the amount of testing time needed to get lower LODs. Using a full beam brings better results in a faster amount of time, increasing throughput for any testing program.
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	No-Worry Service
	

	
	SciAps analyzers are incredibly durable, but every instrument needs maintenance. SciAps offers the lowest service costs in the industry, and we go one step further with a service program that caters to our customers’ needs, across every model, to keep you working at peak performance. Customer service is an extension of our commitment to provide you with exactly what you need, where — and when — you need it.
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	SciAps XRF Full Screening
	

	
	SciAps XRF can be configured for multiple regulations to get the most out of your instrument. Get high throughput and precision for various matrices, all in one testing app.
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	Element
	

	
	RoHS/WEEE
	

	
	CPSIA
	

	
	Halogen Free/ Green
	

	
	Cd
	

	
	<100 ppm
	

	
	Cr
	

	
	Cr6+<1000 ppm
	

	
	Hg
	

	
	<1000 ppm
	

	
	Pb
	

	
	<1000 ppm
	

	
	<100 ppm
	

	
	Br
	

	
	PBB PBDE <1000 ppm
	

	
	<900 ppm
	

	
	Cl
	

	
	<900 ppm
	

	
	50 keV
	

	
	40 keV
	

	
	30 keV
	

	
	Sb
	

	
	Sb2O3 <900 ppm
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	XRF mounted on the Test Station can be operated through SciAps Profile Builder software for PC or tablet to create a benchtop analyzer, allowing you to crank through hundreds of samples a day.
	

	
	SciAps XRF Full Screening
	

	
	Setting up a reasonable screening program allows for rapid testing of the production line. This includes examining incoming material and outgoing QC to assure compliance. While each regulation has its unique requirements for passing and failing products, XRF is a non-destructive technique, so it minimizes the disruption and cost to the product line. Take Pb as an example.
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	For RoHS, Pb pass/fail requirements in a homogenous material are:
	

	
	Pb for RoHS:
	

	
	Pass ≤ 700 – 3σ ≤ Inconclusive ≤ 1300 + 3σ ≤ Fail
	

	
	The Pb action level for RoHS is 1000 ppm. Using XRF for screening, the IEC guidelines put in a 30% buffer for pass/fail that is designated as inconclusive. With XRF, you can neither say it is a pass or fail, and further analysis is required. The inconclusive range also uses the error (σ) associated with the test into expanding the inconclusive region.
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	For CPSIA, it is different:
	

	
	Pb for CPSIA:
	

	
	Pass ≤ 70 – 1σ ≤ Inconclusive ≤ 130 + 1σ ≤ Fail
	

	
	The CPSIA action level for Pb is 100 ppm. Using XRF in accordance with ASTM F2853-10e1 and ASTM 2617-08, there are additional requirements like sample preparation and relative standard deviation of three tests to take into consideration. The extension of the inconclusive zone only uses the error reported (σ) instead of three times that amount. To pass or fail for CPSIA, none of the three tests can fall within the inconclusive zone.
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	All Elements and Matrices
	

	
	Setting up a reasonable screening program allows for rapid testing of the production line. This includes examining incoming material and outgoing QC to assure compliance. While each regulation has its unique requirements for passing and failing products, XRF is a non-destructive technique, so it minimizes the disruption and cost to the product line. Take Pb as an example.
	

	
	50 keV
	

	
	40 keV
	

	
	30 keV
	

	
	15 keV
	

	
	RoHS Plastics
	

	
	Ag, Cd, Sn, Sb, Ba
	

	
	Fe, Co, Ni, Cu, Zn, As, Se, Br, Rb, Sr, Zr, Mo, W, Hg, Tl, Pb, Bi
	

	
	Cl, K, Ca, Tl, V, Mn
	

	
	RoHS Alloy
	

	
	Ag, Cd, Sn, Sb
	

	
	Ti, V, Cr, Mn, Fe, Co, Ni, Cu, Zn, As*, Se, Br, Rb, Sr, Zr, Nb, Mo, W, Au, Hg, Tl, Pb, Bi
	

	
	*Depends on alloy type
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	XRF Compliance Testing Uses
	

	
	With a decade plus of compliance testing experience, SciAps designs instruments to be the fastest and most precise for the growing needs of this market, and Android OS allows for the greatest customization and data management capabilities every time new information becomes available.
	

	
	Further links for XRF and other compliance testing:
	

	
	EU RoHS Directive
	

	
	IPC Halogen Free Website
	

	
	EN 71: Part 3
	

	
	RoHS Testing Website
	

	
	ASTM F963
	

	
	CPSIA
	

	
	ASTM F2617-15
	

	
	REACH Directive
	

	
	EU 94/62/EC Packaging Directive
	

	
	If applicable, please add: 
LOCAL COMPANY NAME
LOCAL WEBSITE
LOCAL PHONE
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World’s lightest, fastest analyzer for ROHS application

The ONLY HH XRF for RoHS, CPSIA, CA Prop 65, Halogen-Free, Environmental Soil

(all RCRAs and EPA Priority Pollutant Metals except Be) and HUD/EPA accepted lead
based paints (X-550 Pb only).

Next-generation connectivity, test data management, barcode reading capabilities,
and reporting for the full range of compliance testing applications, including RoHS,
Halogen Free, CPSIA, and lead paint in children’s playgrounds.
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X-505
Ultimate X-ray Analysis

At 2.75 Ibs,, it's the lightest weight
analyzer ever created, in a mostly
metal frame for ultimate durability
and duty cycle. Perfectly balanced
and fast- you can test material all
day long without fatigue. The
narrow, slender form factor
accesses the toughest test locati-
ons, with the latest 2.7” (68.6mm)
display for rear viewing of chem-
istry.
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X-200
Performance and Value

Competitively priced for every
performance requirement, this
platform weighs about 3.4 lbs.,
making it about 0.5 Ibs. heavier
than the X-550 platform, but still
with industry leading speed and
precision. Updated for improved
heat dissipation, reduced weight,
new user-interface. All internal
electronics now use less power
and operate at higher temper-
atures — no drift or shutdown.
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X-50
Great Basic Analysis

A cost effective SDD detector
processes about 10x lower X-ray
count rates than SDD, resulting in
a 3x reduction of precision. How-
ever, for many RoHS/WEEE app-
lications, the performance is satis-
factory, and the X-50 is available
at a lower price point. Includes the
same advanced X-ray tube (oper-
ating at 50 kV max.), integrated
camera, video, and Android plat-
form.
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Quick, Easy Compliance

XRF is an approved analytical technique for screening various
products for compliance testing, It's the quickest and easiest
way to pass/fail your products.

For RoHS, SciAps instruments comply with IEC 62321-3-1 and
ASTM F2617-15, the official methods that describe procedures
for the analysis of lead, cadmium, chromium, mercury, and total
bromine by XRF. There are additional classifications, like Green
for RoHS, which means complying with RoHS as well as
restricting flame retardants containing Cl, Br and Sb. SciAps
software allows for the ability to add elements like Sb and
adjust pass/fail levels to what the customer requires. SciAps
instruments can also be used in screening for ASTM F963
compliance, an important standard for toy safety.

SciAps engineers have been solving for RoHS from the beginning, through their roles at various companies.
We have decades of experience designing the next generation of instruments to meet the growing needs of
this market. We bring the best possible screening program to our customers based on accuracy, efficiency,
and value for the customer.
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Future-Proof Your Instrument

SciAps RoHS app allows for the greatest customization in the industry. Take back control of
your instrument. As regulations increase, you can add elements like Ni, Sb, Ba, and others.
Want tighter Pass/Fail requirements? Decrease levels to meet your own more stringent
guidelines. No need to buy additional software or a new instrument. Just change settings and

you're ready for any new regulation.

Ease of Use — the ROHS App

With years of experience in the RoHS market, SciAps designs software with the user in mind.
Our automatic identification of material assures that no matter what sample is placed in front
of the window, the results will be right. No need for changing back and forth between different
modes, calibrations, or applications. The simple-to-use RoHS app does it all.
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The Best Value for Your Money
Testing 4 ppm Cd with a Si Pin was unheard of a decade ago. Advancements in digital pulse
processing and the extensive XRF experience at SciAps have produced the best value for
money in the industry. While most instruments in the market have changed very little since
RoHS or CPSIA was first introduced, SciAps newly software takes modern manufacturing into
account.
« State-of-the-art data management incorporated into a flexible Android system allows for
the greatest customization and data management capabilities.
« Redesigned housing with improved heat dissipation allows for high throughput testing that
our compliance customers demand.
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2010 SDD 2010 Si PiN SciAps X-50 PiN
Tube Power 4w 4w 5w
keV 40 keV 40 keV 50 keVv
Max uA 100 uUA 100 uA 200 uA
Detector SDD Si Pin Si Pin

Processing Speed

300-500 MHz CPU,128-500 MB RAM

300-550 MHz CPU,128-500 MB RAM

1.2 GHz CPU,1 GB RAM

Compliance Testing

Testing Time 120 sec 120 sec 60 sec
Typical Alloy Test 120 sec 300 sec 60 sec
LOD: Polymer Pb 2-5 ppm 3-10 ppm 2 ppm
LOD: Polymer Cd 30-50 ppm 30-50 ppm 4 ppm
LOD: Polymer Cr 40-60 ppm 30-60 ppm 2 ppm
LOD: Polymer CI 0.1-0.3% 0.5-1% 60 ppm
LOD: Cu Alloy Cd 60-90 ppm 60-80 ppm 8 ppm
LOD: Sn Alloy Pb 60-90 ppm 120-150 ppm 80 ppm
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Full-Beam Collimation

Why spend more for collimation just to receive 1/8th the power? SciAps XRF tight geometry
and advanced design allows for a 4 mm beam spot without the need for a collimator.
Collimators block X-rays to get the small beam size. This reduces the number of X-rays
going into the samples and thus increases the amount of testing time needed to get lower
LODs. Using a full beam brings better results in a faster amount of time, increasing
throughput for any testing program.
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No-Worry Service

SciAps analyzers are incredibly durable, but every instrument needs maintenance. SciAps
offers the lowest service costs in the industry, and we go one step further with a service
program that caters to our customers’ needs, across every model, to keep you working at
peak performance. Customer service is an extension of our commitment to provide you with
exactly what you need, where — and when — you need it.
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SciAps XRF Full Screening

SciAps XRF can be configured for multiple regulations to get the most out of your instrument.
Get high throughput and precision for various matrices, all in one testing app.
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Element RoHS/WEEE CPSIA Halogen Free/ Green
Cd <100 ppm
Cr Cr6+<1000 ppm
Hg <1000 ppm
Pb <1000 ppm <100 ppm
Br PBB PBDE <1000 ppm <900 ppm
Cl <900 ppm
50 keV 40 keV 30 keV
Sb

Sb203<900 ppm
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XRF mounted on the Test Station can be operated through SciAps Profile Builder software for PC or tablet to
create a benchtop analyzer, allowing you to crank through hundreds of samples a day.

SciAps XRF Full Screening
Setting up a reasonable screening program allows for rapid testing of the
production line. This includes examining incoming material and outgoing
QC to assure compliance. While each regulation has its unique requirements
for passing and failing products, XRF is a non-destructive technique, so it
minimizes the disruption and cost to the product line. Take Pb as an
example.
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For RoHS, Pb pass/fail requirements in a homogenous material are:

Pb for RoHS:
Pass < 700 - 30 < Inconclusive < 1300 + 30 < Fail

The Pb action level for RoHS is 1000 ppm. Using XRF for screening, the IEC guidelines put in a 30% buffer for
pass/fail that is designated as inconclusive. With XRF, you can neither say it is a pass or fail, and further
analysis is required. The inconclusive range also uses the error (o) associated with the test into expanding the

inconclusive region.
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For CPSIA, it is different:

Pb for CPSIA:
Pass < 70 - 10 < Inconclusive < 130 + 1o < Fail

The CPSIA action level for Pb is 100 ppm. Using XRF in accordance with ASTM F2853-10e1 and ASTM 2617-08,
there are additional requirements like sample preparation and relative standard deviation of three tests to take
into consideration. The extension of the inconclusive zone only uses the error reported (o) instead of three
times that amount. To pass or fail for CPSIA, none of the three tests can fall within the inconclusive zone.
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All Elements and Matrices

Setting up a reasonable screening program allows for rapid testing of the production line. This includes
examining incoming material and outgoing QC to assure compliance. While each regulation has its unique

requirements for passing and failing products, XRF is a non-destructive technique, so it minimizes the
disruption and cost to the product line. Take Pb as an example.

50 keV 40 keV 30 keV 15 keV
Fe, Co, Ni, Cu, Zn, As, Se,
RoOHS Plastics | Ag, Cd, Sn, Sb, Ba | Br, Rb, Sr, Zr, Mo, W, Hg, Cl, K, Ca, TI, V, Mn
Tl, Pb, Bi

Ti, V, Cr, Mn, Fe, Co, Ni, Cu,
RoHS Alloy Ag, Cd, Sn, Sb Zn, As*, Se, Br, Rb, Sr, Zr, Nb,

Mo, W, Au, Hg, TI, Pb, Bi

*Depends on alloy type
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XRF Compliance Testing Uses

With a decade plus of compliance testing experience, SciAps designs instruments to be the fastest and most
precise for the growing needs of this market, and Android OS allows for the greatest customization and data
management capabilities every time new information becomes available.

Further links for XRF and other compliance testing: SciAps Inc.
EU RoHS Directive IPC Halogen Free Website EN 71: Part 3 sales@sciaps.com

SciAps.com
RoHS Testing_ Website ASTM F963 +]1 339.927.9455
CPSIA ASTM F2617-15

- Sci’A
REACH Directive EU 94/62/EC Packaging_Directive Cl ps
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RoHS

Halogen-Free and Restricted Substances App

World’s lightest, fastest analyzer for RoHS application
The ONLY HH XRF for RoHS, CPSIA, CA Prop 65, HalogenFree. Environmental Soil
(@il RCRAS and EPA Priorty Politant Metals excest Be) and HUD/EPA sccepted Iead
based paints (X-550 Pb only).

Next-generation comectivity, test data management, barcods reading capabities
and reporting for the full range of compliance testing applcations, ncluding ROHS,
Halogen Frac, CPSIA, and ad paint i chidren's payarounds.
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ROHS

Halogen-Free and Restricted Substances App




