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	The totally re-engineered X-5 offers the industry’s best user interface and ergonomics at a high-value price point. Need optimal performance on precious metals? SciAps powerful, miniaturized X-ray tube, combined with highly advanced internal geometry, yields fast, precise results, delivering in real time the Au, Ag, Pt, and Pd concentrations. Valuable metals are now even more profitable for the precious metals industry.
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	A classic model for many applications at a great value.  
	

	
	Premium X-ray hardware for reliable handling
	

	
	Optimal performance on precious metals like Au, Ag, Pt and Pd
	

	
	Fast, precise results
	

	[image: image5.png]
	X-5
	

	
	XRF
	

	[image: ]
	Optimized handling
	

	
	The X-5 is great for basic analysis of transition and heavy metals. The analyzer includes a built-in, high-resolution camera for photos or video, high-strength polymer mesh to protect the detector, and global connectivity to share results instantly. It also features new internal circuit board, new housing and metal components, up-to-date software and user interface, and full recalibration.
	

	
	Standard element package
	

	
	The X-5 includes the same advanced X-ray tube as other SciAps X Series models (operating at 40 kV max.) for testing including Ti, V, Cr, Mn, Fe, Co, Ni, Cu, Zn, Ir, Pt, Au, Pb, Bi, Zr, Mo, Ru, Rh, Pd, Ag, Cd, Sn, and Sb. More elements can be added upon request.
	

	
	Full sample chemistry—and karat value—
displayed in less than a second. 
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	Android and data management
	

	
	Built on Android OS with the feel of a smart phone and results easily viewed on a vibrant display. Built-in WiFi and USB mean that users can print and email from the X-5 and connect to virtually any information system for real-time data. On-board macro camera allows for photo-documentation of materials tested, and the Bluetooth label printer provides instant hard copy labels.
	

	
	SciAps new test station for the X-5 allows users to analyze small pieces in benchtop mode. Featuring a transparent glass window, the test station allows both buyers and sellers to visually confirm the testing process and view the results in real time.
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	For more information, or to schedule a demonstration: 
	

	
	If applicable, please add: 
LOCAL COMPANY NAME
LOCAL WEBSITE
LOCAL PHONE
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	A classic model for many applications at a great value.
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	Weight
	

	
	2.98 lbs. with battery.
	

	
	Dimensions
	

	
	8.5" x 9.5" x 2.4"
	

	
	Excitation Source
	

	
	4 W, 40 kV Rh Anode X-ray Tube on standard X-5.
	

	
	Detector
	

	
	7 mm2 SDD, silicon drift detector, (active area), 170 eV resolution FWHM at 5.95 Mn K-alpha line.
	

	
	Available Apps
	

	
	Alloy, Precious Metals, Industrial Lead Paint apps. New apps are added regularly, please check with company or website.
	

	
	X-ray Filtering
	

	
	Single primary beam filter
	

	
	Environmental 
Temperature Range
	

	
	10F to 130F at 25% duty cycle.
	

	
	Analytical Range
	

	
	24 elements standard, specific elements vary by app. Ti, V, Cr, Mn, Fe, Co, Ni, Cu, Zn, W, Ta, Hf, Re, Se, Au, Pb, Bi, Zr, Mo, Pd, Ag, Cd, Sn, and Sb. Additional elements may be added upon user request. Precious Metals app is 23 elements standard.
	

	
	Processing Electronics 
and Host Processing
	

	
	1.2 GHz quad ARM Cortex A53 64/32-bit; RAM: 2 GB LP-DDR3; Storage: 16 GB eMMC (storage).
	

	
	Pulse Processor
	

	
	12 bit with digitization rate of 80 MSPS 8K channel MCA USB 2.0 for high-speed data transfer to host processor. Digital filtering implemented in FPGA for high throughput pulse processing, 20 nS - 24 uS peaking time.
	

	
	Power
	

	
	On-board rechargeable Li-ion battery, rechargeable inside device or with external charger, AC power, hot-swap capability (60 s max swap time).
	

	
	Display
	

	
	2.7-inch color capacitive touchscreen — 400 MHz Qualcomm Adreno 306 2D/3D graphics accelerator.
	

	
	Comms/Data Transfer
	

	
	Wi-Fi, Bluetooth, USB connectivity to most devices, including SciAps Profile Builder PC software. 
	

	
	Calibration
	

	
	Fundamental parameters. 
	

	
	Calibration Check
	

	
	External 316 stainless check standard for calibration verification and energy scale validation.
	

	
	Grade Library
	

	
	Standard library contains 500+ grades, no practical size limit. Multiple libraries supported, grades may be added on analyzer or via PC software package (Profile Builder)

	

	
	Security
	

	
	Password protected usage (user level) and internal settings (admin).
	

	
	Dual Cameras
	

	
	Internal high-resolution camera for sample viewing, welds, etc. Macrocamera for photo documentation, reading and storing 2D/3D barcodes and QR codes.
	

	
	Regulatory
	

	
	CE, RoHS, USFDA registered, Canada RED Act.
	

	[image: ]
	YouTube.com/SciAps
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	If applicable, please add: 
LOCAL COMPANY NAME
LOCAL WEBSITE
LOCAL PHONE
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Optimized handling

The X-5 is great for basic analysis of transition and heavy metals. The analyzer
includes a built-in, high-resolution camera for photos or video, high-strength
polymer mesh to protect the detector, and global connectivity to share results
instantly. It also features new internal circuit board, new housing and metal
components, up-to-date software and user interface, and full recalibration.

Standard element package

The X-5 includes the same advanced X-ray tube as other SCiAps X < #100 no crace vt
Series models (operating at 40 kV max.) for testing including Ti, o f @ o
V, Cr, Mn, Fe, Co, Ni, Cu, Zn, Ir, Pt, Au, Pb, Bi, Zr, Mo, Ru, Rh, Pd,
Ag, Cd, Sn, and Sb. More elements can be added upon request.

Full sample chemistry—and karat value—
displayed in less than a second.
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Android and data management

Built on Android OS with the feel of a smart phone and results
easily viewed on a vibrant display. Built-in WiFi and USB mean that
users can print and email from the X-5 and connect to virtually any
information system for real-time data. On-board macro camera
allows for photo-documentation of materials tested, and the
Bluetooth label printer provides instant hard copy labels.

SciAps new test station for the X-5 allows users to analyze small pieces in
benchtop mode. Featuring a transparent glass window, the test station
allows both buyers and sellers to visually confirm the testing process and
view the results in real time.
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For more information, or to
schedule a demonstration:

SciAps Inc.
+1339.927.9455

Sci’Aps




image9.png
A classic model for
many applications
at a great value.
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Available Apps

Environmental
Temperature Range

Analytical Range

Processing Electronics
and Host Processing

Pulse Processor

Comms/Data Transfer

Grade Library

2,98 Ibs. with battery.

85"x95"x 24"

Excitation Source 4 W, 40 kV Rh Anode X-ray Tube on standard X-5.

7 mm? SDD, silicon drift detector, (active area), 170 eV resolution FWHM
at 5.95 Mn K-alpha line.

Alloy, Precious Metals, Industrial Lead Paint apps. New apps are added
regularly, please check with company or website.

Single primary bearn filter

10° F to 130" F at 25% duty cycle.

24 elements standard, specific elements vary by app. Ti, V. Cr, Mn, Fe, Co,
Ni, Cu, Zn, W, Ta, Hf, Re, Se, Au, Pb, Bi, Zr, Mo, Pd, Ag, Cd, Sn, and Sb.
Additional elements may be added upon user request. Precious Metals
app s 23 elements standard.

1.2 GHz quad ARM Cortex AS3 64/32-bit; RAM: 2 GB LP-DDRS; Storage:
16 GB eMMC (storage).

12 bit with digitization rate of 80 MSPS 8K channel MCA USB 2.0 for.
high-speed data transfer to host processor. Digital filtering implemented
in FPGA for high throughput pulse processing, 20 nS - 24 uS peaking
time,

On-board rechargeable Li-ion battery, rechargeable inside device or with
external charger, AC power, hot-swap capability (60 s max swap time).

2.7-inch color capacitive touchscreen — 400 Mz Qualcomm Adreno
306 2D/3D graphics accelerator.

WiFi, Bluetooth, USB connectivity to most devices, including SciAps
Profile Builder PC software,

Fundamental parameters.

External 316 stainless check standard for calibration verification and
energy scale validation.

Standard library contains 500+ grades, no practical size limit. Multiple
libraries supported, grades may be added on analyzer or via PC software
package (Profile Builder)

Password protected usage (user level) and internal settings (admin).
Internal high-resolution camera for sample viewing, welds, etc

Macrocamera for photo documentation, reading and storing 2D/3D.
barcodes and QR codes.

CE, RoHs, USFDA registered, Canada RED Act.
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SciAps Inc.
sales@sciaps.com

SciAps.com
+1 339.927.9455
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‘The totally re-engineered X-5 offers the industry’s best user interface and ergonormics at
a high-value price point. Need optimal performance on precious metals? SciAps
powerful, miniaturized X-ray tube, combined with highly advanced internal geormetry,
yields fast, precise results, delivering in real time the Au, Ag, Pt, and Pd concentrations.
Valuable metals are now even more profitable for the precious metals industry.
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A classic model for
many applications
at a great value.
® Premium X-ray hardware
for reliable handling

@ Optimal performance on
precious metals like Au, Ag,
Ptand Pd

@ Fast, precise results




