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	SciAps X-200 XRF analyzer is the perfect blend of high performance and attractive price. It’s a top-performing SDD with highly optimized X-ray tube and detector geometry, plus improved heat dissipation, reduced weight, and improved durability. Operates on Android OS using Wi-Fi and software with the ease of a smart phone for revolutionary speed, connectivity, and test data management.
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	Totally re-engineered
	

	
	Weighs only 3.1 lbs. with battery
	

	
	Redesigned heat sinking can operate continuously up to 130 °F (54 °C) ambient temperature
	

	
	New internal circuit boards
	

	
	New housing and upgraded metal components
	

	
	Up-to-date software, user interface, and calibration
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	High performance and value
	

	
	The X-200 Series are the lowest priced XRF guns on the market, yet still offer best-in-class analytical and speed performance, with all the accuracy and throughput of SciAps flagship X-550 and X-505.
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	X-ray tube
	

	
	40 kV Rh anode for alloys
	

	
	50 kV Au anode for geochem, soil, RoHS
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	Alloys
	

	
	Fast on every alloy family, SciAps X-200 is a great choice for scrap processing, non-destructive testing and manufacturing quality control.
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	Geochemistry/Soils
	

	
	Industry-comparable precision, LODs and elemental range for environmental, pathfinder, exploration and mining. Analyzers may be factory calibrated with fundamental parameters, Compton Normalization (EPA Method 6200), or user-defined derivative calibrations.
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	RoHS
	

	
	Fast, precise analysis for Pb, Hg, Cd, Br and Cr, plus other restricted materials and Halogen Free requirements. Operates at three beam conditions for optimized LODs across the element suite. Auto‐ mated sample type recognition (polymer, alloy, or mixed type).
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	All internal electronics now use less power and operate at higher temperatures - no delays due to drift or shutdown.
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	For more information, or to schedule a demonstration:
	

	(BACK)
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	Weight
	

	
	3.1 lbs. with battery
	

	
	Dimensions
	

	
	9.38in (238mm) x 11.15in (283mm) x 3.34in (84mm)
	

	
	Power
	

	
	On-board rechargeable Li-ion battery, rechargeable inside device or with external charger, and AC power.
	

	
	Display
	

	
	3.5″ color touch screen, smartphone-type display – PowerVR SGX540 3D graphic
	

	
	Sample Viewing
	

	
	Internal camera for viewing sample before and during analysis for proper sample alignment. Second macro-camera for scanning QR or barcodes and for photo-documentation and report generation.
	

	
	Comms/Data Transfer
	

	

	Wi-Fi, Bluetooth, USB. Connectivity to most devices, including SciAps Profile Builder PC software.
	

	
	Excitation Source
	

	
	5 W X-ray tube. 50 kV max, 200 uA max, Rh or Au anode depending on applic
	

	
	Detector
	

	
	20mm² silicon drift detector (active area), <140eV resolution FWHM at 5.95Mn Kalpha line.
	

	
	X-Ray Filtering
	

	
	6-position filter wheel for beam optimization
	

	
	Processor
	

	
	ARM Cortex -A9 dual-core / 1.2GHz Memory: 1GB DDR2 RAM, 1GB NAND
	

	
	Pulse Processor
	

	
	14-bit ADC with digitization rate of 80 MSPS 8K channel MCA USB 2.0 for high speed data transfer to host processor; digital filtering implemented in FPGA for high throughput pulse processing 50nS – 24uS peaking time
	

	
	Calibration
	

	
	Fundamental Parameters, Compton Normalization, and/or Compton Normalization for Alloy. Geochem, Environmental and Soil calibrations.
	

	
	Calibration Check
	

	
	External 316 stainless check standard for calibration verification and energy scale validation
	

	
	Environmental Temp. Range
	

	
	10°F to 130°F at 25% duty cycle.
	

	
	Security
	

	
	Password protected usage (user level) and internal settings (admin)
	

	
	Regulatory
	

	
	CE, RoHS, USFDA registered, Canada RED Act
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3.1 lbs. with battery

9.38in (238mm) x 11.15in (283mm) x 3.34in (84mm)

On-board rechargeable Li-ion battery, rechargeable inside device or with
external charger, and AC power.

3.5” color touch screen, smartphone-type display - PowerVR SGX540 3D
graphic

Internal camera for viewing sample before and during analysis for proper
sample alignment. Second macro-camera for scanning QR or barcodes
and for photo-documentation and report generation.

Wi-Fi, Bluetooth, USB. Connectivity to most devices, including SciAps
Profile Builder PC software.

5 W X-ray tube. 50 kV max, 200 uA max, Rh or Au anode depending on
application.

20mm? silicon drift detector (active area), <140eV resolution FWHM at
5.95Mn Kalpha line.

6-position filter wheel for beam optimization
ARM Cortex -A9 dual-core / 1.2GHz Memory: 1GB DDR2 RAM, 1IGB NAND
14-bit ADC with digitization rate of 80 MSPS 8K channel MCA USB 2.0 for

high speed data transfer to host processor; digital filtering implemented
in FPGA for high throughput pulse processing 50nS - 24uS peaking time

Fundamental Parameters, Compton Normalization, and/or Compton
Normalization for Alloy. Geochem, Environmental and Soil calibrations.

External 316 stainless check standard for calibration verification and
energy scale validation

10°F to 130°F at 25% duty cycle.

Password protected usage (user level) and internal settings (admin)

CE, RoHS, USFDA registered, Canada RED Act
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SciAps X-200 XRF analyzer is the perfect blend of high performance and
attractive price. It's a top-performing SDD with highly optimized X-ray tube
and detector geometry, plus improved heat dissipation, reduced weight,
and improved durability. Operates on Android OS using Wi-Fi and software
with the ease of a smart phone for revolutionary speed, connectivity, and
test data management.




