
Document Title: SciAps Z-9 Liquidator Specifications
Rev Date: 0823
[image: ]
	Layout Preview
	English Text
	Translated Text

	[image: ]
	SciAps Z-9 Liquidator
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	Results in seconds
	

	
	No dilutions
	

	
	Field-portable
	

	
	Simple! No chemist required
	

	
	Simultaneously measures Li plus B, Na, Mg, K, Ca and more
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	Li Brines Edition
	

	
	SciAps is proud to announce the first portable LIBS powered Lithium Brines analyzer, the Z-9 Liquidator.
	

	
	Combined with the Z-903 handheld LIBS, the Z-9 Liquidator provides fast and easy analysis of brines in the field or in the lab. This groundbreaking technique only needs a 1-2 mL of sample per test, with no dilution necessary. The Z-9 Liquidator samples the liquid and atomizes it into a fine mist which is then analyzed by the Z-903 LIBS. Within seconds, the concentration of Li and other key elements are displayed on nearby tablet or PC.
	

	[image: ]
	World's First In-Field Lithium Brines Analyzer
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	Fast
	

	
	No more waiting days, weeks or even months for results from complicated lab techniques!
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	Easy
	

	
	Simply feed your sample to the Z-9 Liquidator and your brines composition is reported in seconds!
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	Accurate
	

	
	The Z-9 Liquidator is powered by the
SciAps Z-903 handheld LIBS analyzer, equipped with factory built lithium brines calibration. Users can also develop a custom calibration via the Profile Builder software to further optimize performance.
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	Versatile
	

	
	With a small footprint and light but durable construction - the SciAps Z-9
Liquidator is right at home in the lab, in the plant or even in the field! Transportation is easy for analyzing
brines at the well or evaporation ponds.
	

	
	Figure 1: Profile Builder screenshot showing lithium brines results.
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	Have solids or rocks to analyze?
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	Just undock the Z-903 handheld analyzer from the Z-9 Liquidator and you're free to roam! Test outcrops, cores, pressed pellets and more!
	

	
	Calibrations available for pegmatite, Nevada clays, etc.
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Technology
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	SciAps Z-9 Liquidator
	

	
	Specifications
	

	[image: ]
	
	

	[image: ]
	Weight
	

	
	Z-9 Liquidator 15lbs + Z-903 LIBS with
battery 4.93lbs
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	Dimensions
	

	
	9.25" x 11.00" x 16.5"
	

	[image: ]
	Sample Volume
	

	
	~ 1mL per test
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	Analysis Time
	

	
	5s per test
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	Power
	

	

	100-240V, 50/60Hz or optional battery
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	Z-903 Spectral
Range
	

	
	190 - 950 nm
	

	[image: ]
	Drift Correction
	

	
	On-board automated drift correction software with factory-provided or user-provided reference materials
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	Regulatory
	

	
	CE, RoHS, USFDA registered, Safety interlocked Class 3B laser
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	Calibrations
	

	
	Factory built lithium brines calibration or user built calibrations via Profile Builder desktop software
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	Operating
Software
	

	
	SciAps Profile Builder for PC or Windows Tablet
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	YouTube.com/SciAps
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SciAps is proud to announce the first portable LIBS powered Lithium
Brines analyzer, the Z-9 Liquidator.

Combined with the Z-903 handheld LIBS, the Z-9 Liquidator provides
fast and easy analysis of brines in the field or in the lab. This
groundbreaking technique only needs a 1-2 mL of sample per test,
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atomizes it into a fine mist which is then analyzed by the Z-903 LIBS.
‘Within seconds, the concentration of Li and other key elements are

displayed on nearby tablet or PC. d
-





image5.png
World's First In-Field Lithium Brines Analyzer





image6.png
Fast
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Simply feed your sample to the Z-9 Liquidator and your brines
composition is reported in seconds!
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Accurate

The Z-9 Liquidator is powered by the
SciAps  Z-903  handheld  LIBS
analyzer, equipped with factory built
lithium brines calibration. Users can
also develop a custom calibration via
the Profile Builder software to further
optimize performance.
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Just undock the Z-903 handheld analyzer from the Z-9 Liquidator
and you're free to roam! Test outcrops, cores, pressed pellets and
more!

Calibrations available for pegmatite, Nevada clays, etc.
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Sample Volume - 1mL per test
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