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	Industry Challenge
	

	
	Positive Material Identification (PMI) plays a critical role in verifying material compliance across refineries, petrochemical facilities, power generation, fabrication, and manufacturing.
	

	
	SciAps handheld PMI Analyzers such as XRF and LIBS provide rapid alloy verification in the field, but inspection data is often transferred manually after testing. This can delay reporting, increase administrative work, and limit visibility for project managers and quality teams.
	

	
	For applications where carbon is critical to grade identification, inspectors may also need to combine results from complementary technologies and calculate or verify the final grade after testing.
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	Cloud+ Solution
	

	
	Cloud+ creates a connected workflow between SciAps PMI Analyzers and a secure cloud-based platform. Inspection data is automatically synchronized as it is collected, providing a continuously updated backup while making results accessible to authorized personnel.
	

	
	Administrators can manage analyzer fleets remotely, including software updates, configurations, alloy grade libraries, and user access, without requiring analyzers to return to the office.
	

	
	Cloud+ doesn’t just store your data; the Merge Engine combines complementary XRF and LIBS measurements so your inspectors can calculate CE and identify materials on the spot.
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	Workflow
	

	
	Inspectors take measurements with SciAps PMI Analyzers. All data collected is synchronized to Cloud+ constantly, or when Wi-Fi reconnects.
	

	
	Cloud+ can capture and organize:
	

	
	· Material identification results, including chemistry and grade
· Carbon measurements from LIBS 
· Inspection timestamps 
· GPS location 
· Photos and barcodes 
· Analyzer and inspector information 
· Project and custom Test Info fields
	

	
	For multi-sensor applications, Cloud+ Merge Engine combines the carbon results from a SciAps LIBS analyzer with elemental chemistry from a SciAps XRF analyzer. This data fusion can be used to determine CE along with the applicable alloy grade without manually combining measurements or performing calculations after testing.
	

	(BACK)
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	Key Features for NDT/PMI
	

	
	Cloud+ Merge Engine: XRF + Carbon
	

	
	Beyond data storage, the Merge Engine seamlessly combines XRF & LIBS measurements using a “Merge ID” test info value. The software automatically pairs LIBS carbon data with comprehensive XRF chemistry to construct a complete PMI result.
	

	
	For example, when identifying 316 stainless, the LIBS carbon result of 0.03% (Figure 1) is combined with the remaining XRF chemistry to distinguish 316L from standard 316 (Figure 2).
	

	
	This automated data fusion instantly calculates a Grade Match and Carbon Equivalency (CE) in the field. By eliminating manual data entry and disconnected spreadsheets, Cloud+ automates the entire workflow to produce secure traceable reports without the risk of calculation errors.
	

	[image: ]
	Figure 1: Cloud+ provides a secure backup and measurement validation from anywhere.
	

	
	Centralized Inspection Records
	

	
	Cloud+ securely stores inspection history and organizes results using custom fields, making measurements easy to retrieve by project, inspector, analyzer, or other identifying information. Photos, barcodes, GPS coordinates, and chemistry remain associated with the corresponding measurement.
	

	
	Real-Time Data Access
	

	
	Inspection results are available immediately after testing, allowing project managers and quality teams to review data remotely and reducing delays between field testing and reporting.
	

	
	Figure 2: Merge XRF & LIBS data for carbon equivalency, grade ID, and reporting.
	

	
	Remote Administration
	

	
	Manage analyzer fleets without bringing instruments back to the office. Administrators can deploy software updates, maintain consistent analyzer configurations, update alloy grade libraries, and manage user access remotely.
	

	
	Fleet Management
	

	
	Administrators can monitor analyzer health and telemetry, track GPS location, view analyzer usage by inspector login, and manage multiple instruments across facilities.
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	Summary
	

	
	Cloud+ connects SciAps handheld PMI analyzers with a centralized platform for data management, multi-sensor analysis, inspection documentation, and fleet administration.
	

	
	By automatically synchronizing inspection data and combining complementary XRF and LIBS measurements, Cloud+ helps inspectors complete more of the PMI workflow in the field while giving project managers and quality teams greater visibility into inspection activities.
	

	
	Remote fleet management further reduces administrative effort and helps organizations maintain consistent, connected PMI operations across multiple analyzers and facilities.
	

	
	Operational Benefits
	

	
	· Faster PMI Workflows 
· Greater Project Visibility
· Improved Documentation
· Simplified Fleet Management
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Industry Challenge

Positive Material Identification (PMI) plays a critical role in verifying material compliance across refineries,
petrochemical facilities, power generation, fabrication, and manufacturing.

SciAps handheld PMI Analyzers such as XRF and LIBS provide rapid alloy verification in the field, but inspection
data is often transferred manually after testing. This can delay reporting, increase administrative work, and limit
visibility for project managers and quality teams.

For applications where carbon is critical to grade identification, inspectors may also need to combine results
from complementary technologies and calculate or verify the final grade after testing.
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Cloud+ Solution

Cloud+ creates a connected workflow between SciAps PMI Analyzers and a secure cloud-based platform.

Inspection data is automatically synchronized as it is collected, providing a continuously updated backup while
making results accessible to authorized personnel.

Administrators can manage analyzer fleets remotely, including software updates, configurations, alloy grade
libraries, and user access, without requiring analyzers to return to the office.

Cloud+ doesn’t just store your data; the Merge Engine combines complementary XRF and LIBS measurements
so your inspectors can calculate CE and identify materials on the spot.
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Workflow

Inspectors take measurements with SciAps PMI Analyzers. All data collected is synchronized to Cloud+
constantly, or when Wi-Fi reconnects.

Cloud+ can capture and organize:

« Material identification results, including chemistry and grade
e Carbon measurements from LIBS

* Inspection timestamps

* GPS location

* Photos and barcodes

« Analyzer and inspector information

* Project and custom Test Info fields

For multi-sensor applications, Cloud+ Merge Engine combines
the carbon results from a SciAps LIBS analyzer with elemental
chemistry from a SciAps XRF analyzer. This data fusion can be
used to determine CE along with the applicable alloy grade
without manually combining measurements or performing
calculations after testing.
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Key Features for NDT/PMI

Cloud+ Merge Engine: XRF + Carbon

Beyond data storage, the Merge Engine seamlessly combines XRF & LIBS measurements using a “Merge ID” test
info value. The software automatically pairs LIBS carbon data with comprehensive XRF chemistry to construct a
complete PMI result.

For example, when identifying 316 stainless, the LIBS carbon result of 0.03% (Figure 1) is combined with the
remaining XRF chemistry to distinguish 316L from standard 316 (Figure 2).

This automated data fusion instantly calculates a Grade Match and Carbon Equivalency (CE) in the field. By
eliminating manual data entry and disconnected spreadsheets, Cloud+ automates the entire workflow to
produce secure traceable reports without the risk of calculation errors.
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Figure 1: Cloud+ provides a secure backup and measurement
validation from anywhere.

Centralized Inspection Records

Cloud+ securely stores inspection history and organizes
results using custom fields, making measurements easy
to retrieve by project, inspector, analyzer, or other
identifying information. Photos, barcodes, GPS
coordinates, and chemistry remain associated with the
corresponding measurement.

Real-Time Data Access

Inspection results are available immediately after
testing, allowing project managers and quality
teams to review data remotely and reducing
delays between field testing and reporting.

Figure 2: Merge XRF & LIBS data for carbon equivalency,
grade ID, and reporting.

Remote Administration

Manage analyzer fleets without bringing instruments
back to the office. Administrators can deploy
software updates, maintain consistent analyzer
configurations, update alloy grade libraries, and
manage user access remotely.

Fleet Management

Administrators can monitor analyzer health and
telemetry, track GPS location, view analyzer usage
by inspector login, and manage multiple
instruments across facilities.
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Summary

Operational Benefits

Cloud+ connects SciAps handheld PMI analyzers with a
centralized platform for data management, multi-sensor
analysis, inspection documentation, and fleet
administration.

By automatically synchronizing inspection data and
combining complementary XRF and LIBS
measurements, Cloud+ helps inspectors complete more
of the PMI workflow in the field while giving project
managers and quality teams greater visibility into
inspection activities.

Remote fleet management further reduces
administrative effort and helps organizations maintain
consistent, connected PMI operations across multiple
analyzers and facilities.

Faster PMI Workflows

Greater Project Visibility
Improved Documentation
Simplified Fleet Management
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